
[image: image1.png][P)(s]




[image: image2.jpg]


[image: image3.jpg]


[image: image4.jpg]


[image: image5.png]Y




[image: image6.emf]0 1 P

[image: image7.emf]7 0 3

[image: image8.png]


[image: image9.jpg]


[image: image10.emf]A


5. Accessories： 


NO.�
Product name�
Amount�
Product


specification�
Confirm�
�
1�
Electric control box�
1�
�
�
�
2�
Pedal�
1�
PL-313�
�
�
3�
Ballsection connecting rod�
1�
�
�
�
4�
Screw�
3�
M5×25�
�
�
5�
The instructions�
1�
�
�
�
6�
Tensioner�
1�
Lockstitch series clamp/length 35mm,width 25mm/M4�
�
�
7�
Disc head with gasket self-tapping screw�
2�
M3*5�
�
�
8�
Machine head key box�
1�
�
�
�
9�
Fixed plate�
2�
Cold-rolled sheet�
�
�
10�
Fixed plate triple combination connection screw�
2�
M5*20�
�
�
11�
Nut�
2�
M5�
�
�
12�
Thread cutter�
1�
Lockstitch series cutter/double holeΦ3.8�
�
�
13�
Adapter plate�
1�
�
�
�
14�
Hexagon socket fastening screw�
5�
M6*16�
�
�






�





3．Operation Manual：


3.1 Panel Instruction


No.�
button�
description�
�
1�
��
Function key�
�
2�
��
Save key�
�
3�
��
▲：Up key/Up-down needle position compound key�
�
4�
��
▼ ：Down key/Soft start compound key�
�



3.2 Operating mode


3.2.1 Parameter setting


Press P key for 1 second，enter to normal parameter mode, show P01：� EMBED Visio.Drawing.11 ���press▲▼key to change parameter，after press S key, show relevant parameter，press▲▼key to change:� EMBED Visio.Drawing.11 ���


(1) After press S key to save，will show next parameter，press P to exit;


(2) If press P key directly, save the parameter and exit.





2.Parameter Table： 


No�
Project�
Content�
Settingrange�
Thedefault value�
�
1�
Sewing speed�
Set sewing speed�
300～4500 rpm�
3000 rpm�
�
2�
Simple sewing mode Settings�
0：Stopped  1：No stop function�
0/1�
0�
�
3�
Up and down needle position selection�
0：On the needle position  1：Lower needle position�
0/1�
1�
�
4�
Motor rotation�
0：Forward    1：Reversal�
0/1�
0�
�
5�
Soft-start function�
1～10: Soft-start function�
1~10�
2�
�
6�
Soft start speed 1�
speed of the 1st needle of soft start�
300~2000 rpm�
600rpm�
�
7�
Soft start speed 2�
speed of the 2nd needle of soft start�
300~2000 rpm�
1000rpm�
�
8�
Soft start speed 3�
speed of the 3rd~10th needle of soft start�
300~2000 rpm�
1500rpm�
�
12�
Signal mode forturn/lift switch�
Setting of signal mode of turn/lift switch of


machine head 0: always open


1: always close 2:forbid a protection�
0/1/2�
0�
�
13�
Minimum sewing speed�
Minimum sewing speed�
300~1000 rpm�
300rpm�
�
20�
Return to factory-set parameter�
0：Do not restore parameters   1：Restore normal parameters�
0~1�
0�
�
21�
Highest speed of sewing�
highest speed of sewing�
200～4500 rpm�
3000 rpm�
�
31�
Aging speed�
Aging speed�
300～4500 rpm�
3000 rpm�
�
32�
Aging running time�
Aging running time�
1～600ms�
30ms�
�
33�
Aging pause time�
Aging pause time�
1～600ms�
20ms�
�
59�
Down needle positioning position�
To adjust down needle position�
6～18�
12�
�









1. Safety instruction:


Please read the operation manual and related sewing machinery datasheet carefully before correct use.


1.1 (1) Power voltage and frequency: please refer to motor and control box nameplate.


    (2) Interference from electromagnetic wave: please keep far away strong magnetic or high radiation environment in order to avoid obstructions and make to disoperation.


(3) Grounding: to avoid the noise obstructions or leakage of electricity accident (including sewing machine,motor,control box and positioner).


1.2 Please make sure power off at least 1min and then can open control box cover, because there are dangerous high voltage.


1.3 Please turn off the power while repairing or wearing needle in order to protect operator’s safety.


1.4  �Used where potential dangers exist.


�Used where high voltage and electric danger exist.


1.5 If the M6*16 hexagon socket fastening screw comes off, remove it and reinstall it。


1.6 M6*16 hexagon socket fastening screw should be tightened before use. It is not allowed to use without tightening。


1.7 Product warranty period of one year on condition that this machine is operated correctly and no man-made damage.





4.Error Codes:


ErrorCode�
Contents�
Possible reasons�
Checking and treatment�
�
E1�
Hardware drivers fault�
Current detection abnormal


Driving hardware error�
Current detection loop system is working properly;Whether the


damage to the device driver.�
�
E3�
Voltage too high�
Actual high voltage


Voltage detection is wrong�
If the voltage on the inlet wire is too high Whether the system


voltage detection circuit the normal work.�
�
E4�
Voltage too low�
Actual low voltage


Voltage detection is wrong�
If the voltage on the inlet wire is too low Whether the system


voltage detection circuit the normal work.�
�
E7�
Motor HALL signal error�
Motor sensor signal error�
Motor signal detect IC damage or not；�
�
E8�
Motor overload�
Motor stall


motor overload�
If electric engine plug is well contacted;


If machine head or thread-cutting mechanism has been blockedcompletely; if materials are too thick;


Electrical signal detection signal whether the normal.�
�
E11�
HALL A signal lost�
HALL A signal lost�
Motor damage；�
�
E13�
EEPROM error�
Memory IC read abnormal�
Memory IC read abnormal；�
�
E15�
Pedal ID fault�
Pedal verification fault�
Pedal connection is loosen.�
�
E16�
Oz circuit fault�
Oz circuit fault�
Oz circuit system is working properly.�
�
E23�
Down needle position signal error�
Down needle position signal error�
Check down needle sensor damage or not；�
�
E25�
Up needle position signal error�
Up needle position signal error�
Check up needle sensor damage or not；�
�









3.2.2 System Info：


Long press S key for 2 seconds，enter to monitoring mode，press▲▼key to chance monitoring parameter，monitoring value cannot change. Detail monitoring interface see below chart.


show framenumbers�
Item Name�
unit�
�
show framenumbers�
Item Name�
unit�
�
SPD�
speed of motor control�
（*10）rpm�
�
UDC�
Motor Voltage�
V�
�
CUR�
Motor Current�
0.01A�
�
VER�
Voltage�
/�
�



3.2.3 Aging mode：Press P key to enter aging mode，press“P key+▼key” start or stop. system shows：� EMBED Visio.Drawing.11 ���
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