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51.密码设置Password setting


82.格式化CF卡 Format the CF card




   当系统处于“运行”窗口（绿色）时，按按键区域的“准备”按键[image: image1.jpg]


进入操作界面（蓝色窗口），然后按“系统”按键[image: image2.jpg]


进入系统界面。其他情况下直接按“系统”按键[image: image3.jpg]


进入系统界面。

When the system is in the “Run” panel(green), please press the “Ready” Key [image: image4.jpg]


in the key zone to enter the “Operation” panel(blue), then press the “System” key[image: image5.jpg]


, enter into the system interface.While in other interfaces, you can press the “System” key [image: image6.jpg]


directly to enter into the system panel. 
[image: image15.png]6





利用“系统界面”的项[image: image7.png]=



，进入系统管理界面。可以设置密码，设定用户使用期限及格式化CF卡。

   On the [image: image8.png]=



 subclass in the “System” menu,We can set password,set time limit and format CF card.
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1.密码设置Password setting
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在“系统管理界面”按[image: image9.png]6




，我们可以设置各个界面的密码以及对密码进行更改或取消等操作。
Press [image: image10.png]6




 in the “System management” menu, we can set the password for each option , also can  re-set or cancel it.
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2.格式化CF卡 Format the CF card

当出现写入文件出现多次不成功（比如保存花样失败）等CF卡异常情况时请格式化CF卡。
[image: image26.png]


在系统管理界面按[image: image11.png]Rk




按钮，进入密码输入画面。

When you fails to write files for several times(e.g fail to save the design.) or it appears other abnormal situations,please format the CF card.
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Press the [image: image12.png]Rk




 button in the “System management” menu，enter the password inputing interface.

在密码输入画面输入密码，

Input password in the password inputing interface.

输入正确的密码后将显示格式化确认画面。

按确认按钮[image: image13.bmp]进行格式化操作，按取消按钮[image: image14.bmp]则不进行格式化且关闭当前画面。

格式化后显示提示重启的画面。

It shows the format confirm interface if you input the correct password.

格式化完成或者格式化失败时都会出现提示画面要求重启机器。
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It requires to reboot the machine when finishes formating or failed to fomat.

注：格式化重启后进入系统界面和参数界面时需输入密码（初始12345678）

Attention:You must input password when you enter the system interface and the parameter interface(the password is 12345678) after formating and restarting the machine.

各按钮功能：


The function of the buttons:


�：密码设置


    Set password


�：使用期限设置


Set the time limit


�：格式化CF卡


Format the CF card








各按钮功能：


The function of the buttons:


� ：操作界面密码设置


     Password setting in operation interface


� ：参数界面密码设置


Password setting in parameter interface


� ：系统界面密码设置


Password setting in system interface





点击想变更的密码项目按钮，若以前设有密码则需输入密码。


Click the button you want to change the password. You have to input password if you have set .














密码正确后进入密码设置界面


If the password is correct, you will enter the password_setting interface.





在第一个编辑框中输入你想设定的新密码，在第二个编辑框中确认输入的新密码。


按�按钮，新密码确认。


Input the new password in the first edit box, input it again in the second edit box to affirm.


Then press the � button, new password is set.


如果想不设定密码，则让两个编辑框为空并按�按钮即可.


If you don’t want to set any password, you only need make two edit boxes vacancy.
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